Annex No. 1 
 Technical Specification of the Supply
7 pieces of 6 channels data loggers + 10 pieces of 3 channels data loggers 

	Mandatory parameters
	Value
	Parameter accomplished: Yes/No
	Real value

	Sample Rate
	>= 5000 sps
	
	

	Internal Data Storage
	yes
	
	

	Removable Data Storage
	yes
	
	

	Data Type
	miniSEED
	
	

	Streaming Data Format
	SeedLink
	
	

	Ethernet
	yes
	
	

	A/D converter
	>= 24 bit
	
	

	Environmental protection (IP)
	>= 67
	
	

	Mass Centering/Locking/Unlocking
	yes
	
	

	Supply Voltage
	9 – 30 V
	
	

	External GNSS antenna
	yes
	
	




	Rated parameters
	Value
	Parameter accomplished: Yes/No
	Real value
	Maximum Points

	Dynamic Range typical @ 100 sps
	>= 140 dB
	
	
	10

	Size of internal Storage
	>= 8 GB
	
	
	5

	Size of Removable Storage
	>= 32 GB
	
	
	10

	SOH in miniSEED format
	yes
	
	
	3

	Operating Temperature
	<= -20 ˚C
	
	
	10

	Timing Accuracy
	<= 10 us
	
	
	2

	Power Consumption
	<= 1.5 W
	
	
	10

	VPN
	yes
	
	
	5

	Orientation Correction
	yes
	
	
	2





7 pieces of broadband seismometer

	Mandatory parameters
	Value
	Parameter accomplished: Yes/No
	Real value

	Symmetric Triaxial
	yes
	
	

	Force Balance System
	yes
	
	

	Sensitivity
	<= 1000 V/m/s
	
	

	Bandwidth
	10 sec to 100 Hz
	
	

	Velocity Output
	40 V
	
	

	Environmental protection (IP)
	>= 67
	
	

	Supply Voltage
	9 - 30 V
	
	




	Rated parameters
	Value
	Parameter accomplished: Yes/No
	Real value
	Maximum Points

	Clip Level
	>= 20 mm/s
	
	
	10

	Maximum Operating Tilt
	>= 5˚
	
	
	5

	Dynamic Range typical @ 1Hz
	>= 150 dB
	
	
	5

	Power Consumption
	<= 0.5 W
	
	
	10

	Operating Temperature
	<= -20 ˚C
	
	
	10

	Mass Centering required
	no
	
	
	3

























[bookmark: _GoBack]9 pieces of accelerometers


	Mandatory parameters
	Value
	Parameter accomplished: Yes/No
	Real value

	Symmetric Triaxial
	yes
	
	

	Force Balance System
	yes
	
	

	Maximum Full Scale Range
	+-4 g
	
	

	Minimum Full Scale Range
	+-0.25 g
	
	

	Bandwidth
	DC to 200 Hz
	
	

	Acceleration output
	40 V
	
	

	Supply Voltage
	9 - 30 V
	
	

	Environmental protection (IP)
	>= 67
	
	




	Rated parameters
	Value
	Parameter accomplished: Yes/No
	Real value
	Maximum Points

	Dynamic Range typical @ 1Hz
	>= 155 dB
	
	
	10

	Power Consumption
	<= 1.5 W
	
	
	10

	Operating Temperature
	<= -20˚C
	
	
	10





























1 piece of accelerometer with integrated data logger


	Mandatory parameters
	Value
	Parameter accomplished: Yes/No
	Real value

	Symmetric Triaxial
	yes
	
	

	Force Balance System
	yes
	
	

	Maximum Full Scale Range
	+-4 g
	
	

	Minimum Full Scale Range
	+-0.25 g
	
	

	Bandwidth
	DC to 200 Hz
	
	

	Acceleration output
	40 V
	
	

	Supply Voltage
	9 - 30 V
	
	

	Environmental protection (IP)
	>= 67
	
	

	Internal Data Storage
	yes
	
	

	Removable Data Storage
	yes
	
	

	Data Type
	miniSEED
	
	

	Streaming Data Format
	SeedLink
	
	

	Ethernet
	yes
	
	

	A/D converter
	>= 24 bit
	
	

	External GNSS antenna
	yes
	
	



	Rated parameters
	Value
	Parameter accomplished: Yes/No
	Real value
	Maximum Points

	Digitizer Dynamic Range typical @ 100 sps
	>= 140 dB
	
	
	10

	Accelerometer Dynamic Range typical @ 1Hz
	>= 155 dB
	
	
	10

	Size of internal Storage
	>= 8 GB
	
	
	5

	Size of Removable Storage
	>= 32 GB
	
	
	10

	SOH in miniSEED format
	yes
	
	
	3

	Operating Temperature
	<= -20 ˚C
	
	
	10

	Timming Accuracy
	<= 10 us
	
	
	2

	Power Consumption
	<= 3 W
	
	
	10

	VPN
	yes
	
	
	5


Power consumption data logger + broadband seismometer + accelerometer

	Rated parameters
	Value
	Parameter accomplished: Yes/No
	Real value
	Maximum Points

	Power Consumption
	<= 3 W
	
	
	5






